Group-32

Harsh Patel – 100852669

Raquim Dockery 100660304

Christopher Fowler 100711442

Capstone Project DCOM 4100

ISP-3

Table of Contents

[Configuration ISP-3 2](#_Toc163918373)

# Configuration ISP-3

**ISP-3#**

**ISP-3#show run**

**Building configuration...**

**Current configuration : 2807 bytes**

**!**

**! Last configuration change at 23:16:22 UTC Sun Apr 7 2024**

**!**

**version 15.7**

**service timestamps debug datetime msec**

**service timestamps log datetime msec**

**service password-encryption**

**!**

**hostname ISP-3**

**!**

**boot-start-marker**

**boot-end-marker**

**!**

**!**

**!**

**no aaa new-model**

**memory-size iomem 15**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**no ip domain lookup**

**ip domain name ethoca.com**

**ip cef**

**no ipv6 cef**

**!**

**multilink bundle-name authenticated**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**voice-card 0**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**vxml logging-tag**

**license udi pid CISCO2901/K9 sn FGL17302561**

**license accept end user agreement**

**license boot module c2900 technology-package securityk9**

**license boot module c2900 technology-package uck9**

**hw-module pvdm 0/0**

**!**

**!**

**!**

**username admin password 7 104D000A0618**

**!**

**redundancy**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**interface Loopback1**

**ip address 183.32.3.145 255.255.255.240**

**!**

**interface Loopback2**

**ip address 183.32.3.161 255.255.255.240**

**!**

**interface Loopback3**

**ip address 183.32.3.177 255.255.255.240**

**!**

**interface Loopback4**

**description Web Server**

**ip address 192.168.3.5 255.255.255.252**

**ip nat inside**

**ip virtual-reassembly in**

**!**

**interface Loopback5**

**ip address 203.32.1.1 255.255.255.252**

**!**

**interface Embedded-Service-Engine0/0**

**no ip address**

**shutdown**

**!**

**interface GigabitEthernet0/0**

**ip address 123.1.32.34 255.255.255.248**

**ip nat outside**

**ip virtual-reassembly in**

**duplex auto**

**speed auto**

**!**

**interface GigabitEthernet0/1**

**ip address 123.2.32.34 255.255.255.248**

**ip nat outside**

**ip virtual-reassembly in**

**duplex auto**

**speed auto**

**!**

**interface Serial0/1/0**

**no ip address**

**shutdown**

**clock rate 2000000**

**!**

**interface Serial0/1/1**

**no ip address**

**shutdown**

**!**

**router bgp 60323**

**bgp log-neighbor-changes**

**network 123.1.32.32 mask 255.255.255.248**

**network 123.2.32.32 mask 255.255.255.248**

**network 183.32.3.160 mask 255.255.255.240**

**network 183.32.3.160 mask 255.255.255.224**

**network 183.32.3.176 mask 255.255.255.240**

**network 203.32.1.0 mask 255.255.255.252**

**neighbor 123.1.32.33 remote-as 60321**

**neighbor 123.2.32.33 remote-as 60322**

**!**

**ip forward-protocol nd**

**!**

**no ip http server**

**no ip http secure-server**

**!**

**ip nat inside source static 192.168.3.5 203.32.1.1**

**ip ssh version 2**

**!**

**!**

**!**

**!**

**control-plane**

**!**

**!**

**voice-port 0/2/0**

**!**

**voice-port 0/2/1**

**!**

**voice-port 0/3/0**

**!**

**voice-port 0/3/1**

**!**

**!**

**!**

**!**

**!**

**mgcp behavior rsip-range tgcp-only**

**mgcp behavior comedia-role none**

**mgcp behavior comedia-check-media-src disable**

**mgcp behavior comedia-sdp-force disable**

**!**

**mgcp profile default**

**!**

**!**

**!**

**!**

**!**

**!**

**!**

**gatekeeper**

**shutdown**

**!**

**banner login ^CUnauthorized access to this device is prohibited!^C**

**banner motd ^CUnauthorized access to this device is prohibited!^C**

**!**

**line con 0**

**logging synchronous**

**login local**

**transport output ssh**

**stopbits 1**

**line aux 0**

**exec-timeout 0 0**

**no exec**

**transport output none**

**line 2**

**no activation-character**

**no exec**

**transport preferred none**

**transport output pad telnet rlogin lapb-ta mop udptn v120 ssh**

**stopbits 1**

**line vty 0 4**

**login local**

**transport input ssh**

**transport output ssh**

**line vty 5 15**

**exec-timeout 5 0**

**login local**

**transport input ssh**

**transport output ssh**

**!**

**scheduler allocate 20000 1000**

**!**

**end**

**ISP-3#$**

**ISP-3#**

**ISP-3#**